**Pinouts:**

|  |  |
| --- | --- |
| **Pin on RELAY** | **Description** |
| VCC | 5V |
| GND | Ground |
| Data pin | “1” or “0” from microcontroller |
| NC | For Normally Closed Circuit |
| COM | Common |
| NO | For Normally Open Circuit |

|  |  |
| --- | --- |
| **Pin on HC-05** | **Description** |
| EN/key | High – Command Mode, Low – Data Mode |
| VCC | 3.3 V to 5 V |
| GND | Ground |
| TXD | Transmit Serial Data |
| RXD | Receive Serial Data |
| State | Shows module connected or not |